Thanks for purchasing your Mac compatible Wireless N PCI Card

Disregard the CD that came with the card.  It is an installer for PC's.

Open your computer and locate an open PCI slot.  Remove the screw holding down the cover. The card will snap down in the slot squarely.  Replace the screw.

Install the external antennas.  Straighten them out to thread in.

Install the appropriate driver for your OS version.

Once you reboot your computer, select System Preference/Network.  Select the PCI slot you installed the card in. It should automatically recognize the new device and walk you through configuring it for your network.

Use the installed RA Link software to configure for connecting to your wireless network. Select add to profile if you need to set up for encryption. Setting up the profile also saves your settings so you don't have to repeat it.

Operator Headgap Systems, Inc.
http://headgapstore.com