Thanks for purchasing your Mac compatible Wireless G USB Dongle

Disregard the CD that came with the card.  It is an improper size to use in a Mac.

Install the appropriate driver for your OS version.  Use the Tiger installer for Leopard.  We have tested it. The 8187B uses a different driver.

Once you reboot your computer, select System Preference/Network.  It should automatically recognize the new device and walk you through configuring it for your network.

Please NOTE:  The driver for the RTL8187B Chipset is for Tiger and Leopard ONLY.

Operator Headgap Systems, Inc.
http://headgapstore.com